AC RESISTER CONTROL

LOAD OF AC:

D0T5: AC🡨AC^DR

D1T5: AC🡨AC+DR

D2T5­: AC🡨DR

D7I’T3B11: AC🡨AC’

D7I’T3B7: AC🡨shr AC, AC(15)🡨E

D7I’T3B6: AC🡨shl AC, AC(0)🡨E

D7IT3B11: AC(0-7)🡨INPR

CLEAR OF AC:

D7I’T3B11: AC🡨0

INCREAMENT OF PC:

D7I’T3B5: AC🡨AC+1