OUTR RESISTER CONTROL

LOAD OF OUTR:

D7IT3B10: OUTR🡨AC(0-7)