TR RESISTER CONTROL

LOAD OF TR:

RT0: TR🡨PC